Table 3. Plugin parameter settings for performance tests

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Parameter Name | All we know | In the name of Love | Closer |
| 1 | Tempo (bpm) | 90 | 134 | 95 |
| 2 | Bypass | Off | Off | Off |
| 3 | Threshold 1 (dB) | -20.44 | -28.897 | -10.97 |
| 4 | Decay Time 1 (ms) | 10 | 10 | 10 |
| 5 | Mix 1 (ratio) | 1 | 1 | 1 |
| 6 | Envelope Control Attack 1 (sec) | 0.01 | 0.01 | 0.1 |
| 7 | Envelope Control Sustain 1 (count) | 0.75 | 3 | 0.5 |
| 8 | Envelope Control Release 1 (sec) | 0.07 | 0.07 | 0.27 |
| 9 | LFO Control Floor 1  | Off | Off | Off |
| 10 | LFO Control Frequency 1 | Off | Off | Off |
| 11 | LFO Control Invert 1 | Off | On | Off |
| 12 | LFO Control Count 1 | 4 | 1 | - |
| 13 | LFO Control Shape 1 | Sine | Sine | - |
| 14 | Amp Mod On/Off 1 | On | On | On |
| 15 | Amp Mod LFO 1 | On | On | Off |
| 16 | Amp Mod Depth 1 (ratio) | 1 | 1 | 1 |
| 17 | Filter On/Off 1  | Off | Off | Off |
| 18 | Filter Select 1 | - | - | - |
| 19 | Filter Depth 1 (Hz) | - | - | - |
| 20 | Threshold 2 (dB) | 0 | -19.261 | -18.782 |
| 21 | Decay Time 2 (ms) | - | 10 | 10 |
| 22 | Mix 2 (ratio) | - | 1 | 1 |
| 23 | Envelope Control Attack 2 (sec) | 0 | 0 | 0.1 |
| 24 | Envelope Control Sustain 2 (count) | 0 | 0.125 | 0.5 |
| 25 | Envelope Control Release 2 (sec) | 0 | 0 | 0.27 |
| 26 | LFO Control Floor 2 | - | Off | Off |
| 27 | LFO Control Frequency 2 | - | Off | Off |
| 28 | LFO Control Invert 2 | - | Off | Off |
| 29 | LFO Control Count 2 | - | - | - |
| 30 | LFO Control Shape 2 | - | - | - |
| 31 | Amp Mod On/Off 2 | - | Off | On |
| 32 | Amp Mod LFO 2 | - | Off | Off |
| 33 | Amp Mod Depth 2 (ratio) | - | 0 | 1 |
| 34 | Filter On/Off 2 | - | Off | Off |
| 35 | Filter Select 2 | - | - | - |
| 36 | Filter Depth 2 (Hz) | - | 0 | - |